Building configuration...


  
  
  
Current configuration : 23900 bytes
!
! Last configuration change at 17:53:29 YEKT Mon Jul 4 2022 by adm_kapustinal
! NVRAM config last updated at 17:57:40 YEKT Mon Jul 4 2022 by adm_kapustinal
!
version 15.7
service timestamps debug datetime msec localtime show-timezone year
service timestamps log datetime msec localtime show-timezone year
no service password-encryption
service internal
!
hostname PRM-MLK-PHK-RT-1-1
!
boot-start-marker
boot system flash:c2900-universalk9-mz.SPA.157-3.M.bin
boot-end-marker
!
!
logging userinfo
logging buffered 128000
enable secret 5 $1$QW0D$QYciH.O0GY9GW37Ao2khP1
!
aaa new-model
!
!
aaa group server radius NPS
 server name IZH-RDS002
 server name P11-RDS003
 ip radius source-interface GigabitEthernet0/0.300
 load-balance method least-outstanding
!
aaa authentication login default group NPS local enable
aaa authentication login CONSOLE local group NPS
aaa authentication ppp default local
aaa authorization exec default group NPS local if-authenticated 
!
!
!
!
!
aaa session-id common
no process cpu extended history
no process cpu autoprofile hog
clock timezone YEKT 5 0
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!


!
ip vrf AUX
!
!
!
!
ip flow-cache timeout inactive 60
ip flow-cache timeout active 5
no ip domain lookup
ip domain name milkom-komos.ru
ip host tftp 10.4.0.214
ip name-server 8.8.8.8
ip inspect WAAS flush-timeout 10
ip inspect tcp reassembly queue length 128
ip inspect tcp reassembly timeout 10
ip inspect name INTERNET tcp router-traffic
ip inspect name INTERNET udp router-traffic
ip inspect name INTERNET icmp router-traffic
ip cef
login on-failure log
login on-success log
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
crypto pki trustpoint test2
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-2171384109
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-2171384109
 revocation-check none
 rsakeypair TP-self-signed-2171384109
!
!
crypto pki certificate chain test2
crypto pki certificate chain TP-self-signed-2171384109
 certificate self-signed 01
  3082022B 30820194 A0030201 02020101 300D0609 2A864886 F70D0101 04050030 
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 32313731 33383431 3039301E 170D3138 31323034 31313332 
  30385A17 0D323030 31303130 30303030 305A3031 312F302D 06035504 03132649 
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D32 31373133 
  38343130 3930819F 300D0609 2A864886 F70D0101 01050003 818D0030 81890281 
  8100E149 A4415C28 ED01D327 225DDA3A CBCC8201 BBCD66CC F547B862 F96ABF51 
  ECA28654 A51FBDB6 BE535596 1A243475 4EDBD970 A609A77F 6B3430C9 470CD0AC 
  D2ED7036 EFED3FD6 C859496E 5BFC22E9 E7A0D1CC 8F0A4D81 4BDB56AA F6785341 
  4A8C205C B8D00236 7CE71518 C92D846A 75B7A96C 216050B9 35A46069 8243269D 
  E82F0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF 301F0603 
  551D2304 18301680 14BD2B4F 3437D9F4 BBCE670B AB70193E 34F8BC03 15301D06 
  03551D0E 04160414 BD2B4F34 37D9F4BB CE670BAB 70193E34 F8BC0315 300D0609 
  2A864886 F70D0101 04050003 81810023 D7C7944F 5DC995CB 6B907110 B8B86DD9 
  0A66F4AD E01A03A0 97860857 0BA76294 2EE20C59 99603325 9AB0E274 C20A43DC 
  D2FCB98A 6E4286B4 25C7170E E0BF9799 AD8E6A1B 9B8ACBBE 743C4136 C67632BF 
  120DCE48 F6887715 6253CE9B 3A3784CE 2895C5C2 3867F61C FF519239 FAA315FD 
  1BA28FD7 CE7671CE 5E917E38 4E5184
  	quit
voice-card 0
!
!
!
!
!
!
!
!
license udi pid CISCO2911/K9 sn FJC1940A2Q2
license accept end user agreement
license boot module c2900 technology-package securityk9
license boot module c2900 technology-package uck9
license boot module c2900 technology-package datak9
!
!
archive
 log config
  logging enable
  logging size 900
  notify syslog contenttype plaintext
  hidekeys
 path tftp://tftp/PHK/2911/$H-$T
 write-memory
 time-period 10080
object-group network OBJ_BBN_RN_BBN 
 host 85.140.32.104
 host 78.85.13.205
!
object-group network OBJ_BBN_VST_BBN 
 host 85.140.32.103
 host 83.169.220.204
!
object-group network OBJ_IZH_MLK_IZM 
 host 85.140.32.27
 host 78.85.13.42
 host 5.227.126.169
 host 31.173.105.54
 host 217.14.195.253
 host 85.175.86.74
!
object-group network OBJ_IZH_KG_P11 
 91.240.179.0 255.255.255.0
 host 5.227.124.143
 host 78.85.13.93
 host 62.141.96.126
 host 84.201.247.190
 host 88.80.33.50
 host 94.25.46.122
!
object-group network OBJ_IZH_VST_IZM 
 host 5.227.124.82
 host 78.85.13.38
!
object-group network OBJ_IZH_TK_M44 
 host 212.46.204.74
 host 88.80.33.162
!
object-group network OBJ_IZH_TK_M48 
 host 87.249.237.250
!
object-group network OBJ_IZH_TK_SMR 
 host 87.249.239.226
 host 88.80.33.42
!
object-group network OBJ_MSK_KG_MSK 
 host 185.62.195.150
 host 185.6.175.101
!
object-group network OBJ_GLZ_MLK_GMK 
 host 31.173.105.62
 host 85.140.32.29
!
object-group network OBJ_KZN_MLK_KMK 
 host 83.69.126.54
 host 94.180.253.210
 host 78.138.171.82
!
object-group network OBJ_KEZ_MLK_KZS 
 host 31.173.105.66
 host 78.85.13.52
 host 85.140.32.30
!
object-group network OBJ_PRM_MLK_PHK 
 host 178.47.128.18
 host 46.146.210.68
!
object-group network OBJ_SAR_MLK_SRM 
 host 31.173.105.58
 host 78.85.13.53
 host 85.140.32.28
!
object-group network OBJ_CLB_MLK_CMK 
 host 37.113.128.241
 host 149.255.6.35
!
object-group network OBJ_GLZ_GKZ_GKZ 
 host 78.85.13.94
 host 146.120.104.181
!
object-group network OBJ_KIA_RN_KIA 
 host 78.85.14.97
!
object-group network OBJ_IZH_TZK_TZK 
 host 78.25.80.134
 host 5.227.124.235
!
object-group network OBJ_IZH_MK_VS17 
 host 5.227.124.141
!
object-group network OBJ_IZH_KL_KLI 
 host 78.85.15.85
 host 84.201.247.24
 host 79.175.36.97
 host 84.201.244.235
!
object-group network OBJ_EKB_KG_EKB 
 host 62.168.232.182
 host 176.215.14.11
!
object-group network OBJ_IZH_KEN_VS56 
 host 83.143.54.246
 host 92.55.54.109
!
object-group network OBJ_IZH_VRS_IZM 
 host 85.140.32.177
 host 78.85.14.98
!
object-group network OBJ_GLZ_VRS_UPF 
 host 95.215.208.234
 host 78.85.13.119
!
object-group network OBJ_IZH_VRS_IPF 
 host 85.140.32.141
 host 78.85.13.117
!
object-group network OBJ_IZH_VRS_PFV 
 host 85.140.32.178
 host 94.181.119.90
 host 78.85.33.50
!
object-group network OBJ_VOT_VRS_VPF 
 host 78.85.13.118
 host 88.80.33.14
!
object-group network OBJ_MSB_TMA_MSB 
 host 78.138.182.214
!
object-group network OBJ_KIB_TMA_KIB 
 host 78.138.182.126
!
object-group network OBJ_PRM_VRS_MPF 
 host 178.47.130.10
 host 5.227.121.127
!
object-group network OBJ_LAI_VRS_DPF 
 host 178.205.241.114
 host 46.232.164.108
!
object-group network OBJ_SHM_TMA_SHM 
 host 89.232.91.106
 host 31.173.182.210
!
object-group network OBJ_EVL_TMA_EVL 
 host 89.232.102.166
!
object-group network OBJ_ITL_VST_ITL 
 host 5.227.124.130
 host 78.85.34.99
 host 81.211.13.82
!
object-group network OBJ_MZH_VST_MZH 
 host 88.80.33.250
 host 83.169.220.171
!
object-group network OBJ_KIA_VST_KIA 
 host 85.140.32.24
 host 188.94.168.238
!
object-group network OBJ_KGB_VST_KBB 
 host 78.85.37.88
 host 88.80.33.154
!
object-group network OBJ_SAR_VST_SMK 
 host 78.85.19.93
 host 88.80.33.234
!
object-group network OBJ_KNK_VST_KMK 
 host 178.161.242.67
!
object-group network OBJ_IZH_KM_S61 
 host 84.201.247.32
 host 88.80.33.194
!
object-group network OBJ_YAN_GKZ_YEL 
 host 77.94.97.222
!
object-group network OBJ_KUN_KMK_B2 
 94.138.150.0 255.255.255.0
!
object-group network OBJ_KUN_KMK_H80 
 host 178.161.207.26
 host 77.43.193.88
!
object-group network OBJ_KUN_KMK_CH9 
 host 178.47.128.98
 host 194.150.90.20
!
object-group network OBJ_KGB_RN_KGB 
 host 78.85.13.165
!
object-group network OBJ_NCH_RN_NCH 
 host 78.85.13.166
!
object-group network OBJ_PRI_RN_PRI 
 host 78.85.13.167
!
object-group network OBJ_URN_RN_URN 
 host 78.85.20.49
!
object-group network OBJ_MZH_TK_TKM 
 host 88.80.32.230
 host 78.85.35.34
!
object-group network OBJ_GLZ_TK_TKG 
 host 95.215.208.240
 host 146.120.104.235
 host 95.215.208.173
!
object-group network OBJ_IZH_TK_M21 
 host 84.201.242.133
!
object-group network OBJ_IZH_HLA_PP 
 host 92.61.17.250
!
object-group network OBJ_IZH_HLA_UHK 
 host 92.55.7.148
!
object-group network OBJ_IZH_VD_VS17 
 host 84.201.247.100
!
object-group network OBJ_IZH_KS_H17 
 85.140.32.64 255.255.255.252
 host 85.140.32.63
 host 85.140.32.68
!
object-group network OBJ_IZH_KI_VOR158 
 host 46.147.130.59
 host 5.227.125.126
!
object-group network OBJ_SPB_KG_SPB 
 host 62.141.114.190
 host 94.72.27.43
!
object-group network OBJ_BRANCHES 
 group-object OBJ_IZH_MLK_IZM
 group-object OBJ_IZH_KG_P11
 group-object OBJ_IZH_VST_IZM
 group-object OBJ_IZH_TK_M44
 group-object OBJ_IZH_TK_M48
 group-object OBJ_IZH_TK_SMR
 group-object OBJ_MSK_KG_MSK
 group-object OBJ_GLZ_MLK_GMK
 group-object OBJ_KZN_MLK_KMK
 group-object OBJ_KEZ_MLK_KZS
 group-object OBJ_PRM_MLK_PHK
 group-object OBJ_SAR_MLK_SRM
 group-object OBJ_CLB_MLK_CMK
 group-object OBJ_BBN_RN_BBN
 group-object OBJ_GLZ_GKZ_GKZ
 group-object OBJ_KIA_RN_KIA
 group-object OBJ_IZH_TZK_TZK
 group-object OBJ_IZH_MK_VS17
 group-object OBJ_IZH_KL_KLI
 group-object OBJ_EKB_KG_EKB
 group-object OBJ_IZH_KEN_VS56
 group-object OBJ_IZH_VRS_IZM
 group-object OBJ_GLZ_VRS_UPF
 group-object OBJ_IZH_VRS_IPF
 group-object OBJ_IZH_VRS_PFV
 group-object OBJ_VOT_VRS_VPF
 group-object OBJ_MSB_TMA_MSB
 group-object OBJ_KIB_TMA_KIB
 group-object OBJ_PRM_VRS_MPF
 group-object OBJ_LAI_VRS_DPF
 group-object OBJ_BBN_VST_BBN
 group-object OBJ_SHM_TMA_SHM
 group-object OBJ_EVL_TMA_EVL
 group-object OBJ_ITL_VST_ITL
 group-object OBJ_MZH_VST_MZH
 group-object OBJ_KIA_VST_KIA
 group-object OBJ_KGB_VST_KBB
 group-object OBJ_SAR_VST_SMK
 group-object OBJ_KNK_VST_KMK
 group-object OBJ_IZH_KM_S61
 group-object OBJ_YAN_GKZ_YEL
 group-object OBJ_KUN_KMK_B2
 group-object OBJ_KUN_KMK_H80
 group-object OBJ_KUN_KMK_CH9
 group-object OBJ_KGB_RN_KGB
 group-object OBJ_NCH_RN_NCH
 group-object OBJ_PRI_RN_PRI
 group-object OBJ_URN_RN_URN
 group-object OBJ_MZH_TK_TKM
 group-object OBJ_GLZ_TK_TKG
 group-object OBJ_IZH_TK_M21
 group-object OBJ_IZH_HLA_PP
 group-object OBJ_IZH_HLA_UHK
 group-object OBJ_IZH_VD_VS17
 group-object OBJ_IZH_KS_H17
 group-object OBJ_IZH_KI_VOR158
 group-object OBJ_SPB_KG_SPB
!
object-group network ROUTETOISP1 
 host 192.168.51.101
 host 192.168.20.251
!
object-group network ROUTETOISP2 
 host 192.168.51.99
!
object-group network STATIC_ISP_IP 
 host 46.146.210.68
 host 178.161.175.54
 host 178.47.128.18
!
object-group service SVC_ANDROMEDA 
 tcp eq 47623
!
object-group service SVC_APS 
 tcp eq 48718
!
object-group service SVC_APS2 
 tcp eq 48608
!
object-group service SVC_IM 
 tcp eq 10883
 udp eq 10883
!
object-group service SVC_IPTel 
 udp eq 5060
 tcp eq 5060
 udp eq 35060
 udp range 16000 16999
 tcp range 12000 12255
 udp range 12000 12255
!
object-group service SVC_MAIL 
 tcp eq smtp
 tcp eq pop3
 tcp eq 143
 tcp eq 465
 tcp eq 993
 tcp eq 995
!
object-group service SVC_POLYCOM 
 tcp-udp eq 1720
 tcp-udp eq 3230
 tcp-udp eq 3232
 tcp-udp eq 3231
 tcp-udp eq 3233
 tcp-udp eq 3234
 tcp-udp eq 3235
!
object-group service SVC_SYSADM 
 tcp eq 40688
!
object-group service SVC_VideoServer 
 tcp eq 37395
 udp eq 37395
!
object-group network USER_APS2 
 host 92.61.17.250
 host 92.55.7.148
!
object-group service VIDEO-TEMP 
 tcp eq 34501
 tcp eq 34502
 tcp eq 34503
!
username netadmin privilege 15 secret 5 $1$0bIn$C5O/.4AvGkm8LuXS4WK2D.
!
redundancy
 notification-timer 120000
!
!
!
!
!
track 1 ip sla 1 reachability
 delay down 10 up 5
!
track 2 ip sla 2 reachability
 delay down 10 up 5
!
track 3 ip sla 3 reachability
 delay down 10 up 5
!
track 4 ip sla 4 reachability
 delay down 10 up 5
!
track 5 ip sla 5 reachability
 delay down 10 up 5
!
track 6 ip sla 6 reachability
 delay down 10 up 5
!
track 10 list boolean or
 object 1
 object 2
 object 3
 object 4
 object 5
 object 6
 delay down 5 up 30
!
! 
!
crypto isakmp policy 150
 encr aes
 authentication pre-share
 group 2
crypto isakmp key mlk20kom19 address 0.0.0.0         no-xauth
crypto isakmp keepalive 30
crypto isakmp nat keepalive 10
!
!
crypto ipsec transform-set TS_DMVPN esp-aes esp-sha-hmac 
 mode transport
!
crypto ipsec profile IPSEC_DMVPN
 description -==SPOKE to SITE DMVPN IPSec GRE Profile ==-
 set transform-set TS_DMVPN 
!
!
!
!
!
!
!
interface Loopback777
 description AUX
 ip vrf forwarding AUX
 ip address 10.255.255.255 255.255.255.255
!
interface Tunnel1001
 description DMVPN_SPOKE6_Cloud1
 bandwidth 30000
 ip address 172.30.1.11 255.255.255.0
 ip access-group ACL_TO_DMVPN out
 no ip redirects
 ip mtu 1400
 ip flow ingress
 ip nhrp authentication M_K.Cl01
 ip nhrp map 172.30.1.1 85.140.32.27
 ip nhrp map 172.30.1.2 78.85.13.42
 ip nhrp map multicast 85.140.32.27
 ip nhrp map multicast 78.85.13.42
 ip nhrp network-id 1001
 ip nhrp holdtime 300
 ip nhrp nhs 172.30.1.1
 ip nhrp nhs 172.30.1.2
 ip tcp adjust-mss 1360
 tunnel source GigabitEthernet0/1
 tunnel mode gre multipoint
 tunnel key 1001
 tunnel protection ipsec profile IPSEC_DMVPN shared
!
interface Tunnel1002
 description DMVPN_SPOKE6_Cloud2
 bandwidth 30000
 ip address 172.30.2.11 255.255.255.0
 ip access-group ACL_TO_DMVPN out
 no ip redirects
 ip mtu 1400
 ip flow ingress
 ip nhrp authentication M_K.Cl02
 ip nhrp map 172.30.2.2 78.85.13.93
 ip nhrp map 172.30.2.1 5.227.124.143
 ip nhrp map multicast 5.227.124.143
 ip nhrp map multicast 78.85.13.93
 ip nhrp network-id 1002
 ip nhrp holdtime 300
 ip nhrp nhs 172.30.2.1
 ip nhrp nhs 172.30.2.2
 ip tcp adjust-mss 1360
 tunnel source GigabitEthernet0/1
 tunnel mode gre multipoint
 tunnel key 1002
 tunnel protection ipsec profile IPSEC_DMVPN shared
!
interface Null0
 no ip unreachables
!
interface Embedded-Service-Engine0/0
 no ip address
 shutdown
!
interface GigabitEthernet0/0
 no ip address
 duplex auto
 speed auto
!
interface GigabitEthernet0/0.111
 description INTERCONNECT
 encapsulation dot1Q 111
 ip address 172.16.5.1 255.255.255.248
 no ip redirects
 no ip unreachables
 no ip proxy-arp
 ip flow ingress
 ip flow egress
 ip nat inside
 ip virtual-reassembly in
 standby version 2
 standby 1 ip 172.16.5.3
 standby 1 priority 120
 standby 1 preempt
 standby 1 name VSS
 standby 1 track 10 decrement 20
 ip policy route-map GLOBAL-ROUTING
!
interface GigabitEthernet0/0.300
 description --MANAGEMENT--
 encapsulation dot1Q 300
 ip address 10.5.126.251 255.255.255.0
 no ip redirects
 no ip unreachables
 no ip proxy-arp
 ip flow ingress
 ip flow egress
 ip nat inside
 ip virtual-reassembly in
!
interface GigabitEthernet0/0.555
 description --BGP_TRANSIT--
 encapsulation dot1Q 555
 ip address 172.30.30.92 255.255.255.248
 no ip redirects
 no ip unreachables
 no ip proxy-arp
 ip flow ingress
 ip flow egress
!
interface GigabitEthernet0/1
 description [30M] --ERTELECOM--
 ip address 46.146.210.68 255.255.255.0
 ip access-group FIREWALL in
 ip flow ingress
 ip nat outside
 ip inspect INTERNET out
 ip virtual-reassembly in max-reassemblies 256
 duplex auto
 speed auto
 no cdp enable
 no mop enabled
!
interface GigabitEthernet0/2
 no ip address
 shutdown
 duplex auto
 speed auto
!
!
router bgp 64517
 bgp router-id 172.30.30.92
 bgp log-neighbor-changes
 bgp graceful-restart
 network 10.5.126.0 mask 255.255.255.0
 neighbor 172.30.1.1 remote-as 64512
 neighbor 172.30.1.1 soft-reconfiguration inbound
 neighbor 172.30.1.1 route-map RM_TO_HUB out
 neighbor 172.30.1.2 remote-as 64512
 neighbor 172.30.1.2 soft-reconfiguration inbound
 neighbor 172.30.1.2 route-map RM_TO_HUB out
 neighbor 172.30.2.1 remote-as 64513
 neighbor 172.30.2.1 soft-reconfiguration inbound
 neighbor 172.30.2.1 route-map RM_TO_HUB out
 neighbor 172.30.2.2 remote-as 64513
 neighbor 172.30.2.2 soft-reconfiguration inbound
 neighbor 172.30.2.2 route-map RM_TO_HUB out
 neighbor 172.30.30.93 remote-as 64517
 neighbor 172.30.30.93 next-hop-self all
 neighbor 172.30.30.93 soft-reconfiguration inbound
 neighbor 172.30.30.94 remote-as 64517
 neighbor 172.30.30.94 next-hop-self all
 neighbor 172.30.30.94 soft-reconfiguration inbound
 distance bgp 150 150 150
!
ip local policy route-map RM_LOCAL
ip forward-protocol nd
!
no ip http server
ip http access-class 23
no ip http secure-server
ip http timeout-policy idle 60 life 86400 requests 10000
ip flow-export source GigabitEthernet0/0.300
ip flow-export version 5
ip flow-export destination 192.168.51.99 9996
ip flow-export destination 10.4.0.215 9995
ip flow-top-talkers
 top 10
 sort-by packets
 cache-timeout 10000
!
ip tftp source-interface GigabitEthernet0/0.300
ip nat translation timeout 450
ip nat translation tcp-timeout 300
ip nat translation pptp-timeout 1800
ip nat translation udp-timeout 45
ip nat translation dns-timeout 5
ip nat translation port-timeout tcp 110 60
ip nat translation port-timeout tcp 25 60
ip nat translation port-timeout tcp 80 15
ip nat translation max-entries all-host 400
ip nat inside source route-map ISP_1 interface GigabitEthernet0/1 overload
ip nat inside source route-map ISP_2 interface GigabitEthernet0/2 overload
ip nat inside source static tcp 192.168.52.191 7010 178.47.128.18 7010 extendable
ip nat inside source static tcp 192.168.52.192 7020 178.47.128.18 7020 extendable
ip route 0.0.0.0 0.0.0.0 46.146.210.254 50 name --ERTELECOM--
ip route 10.0.0.0 255.255.255.0 172.16.5.4 200 name --PROD_MARKLINE--
ip route 10.5.112.0 255.255.255.224 172.16.5.4 200 name --OOO_SOZVEZDIE--
ip route 10.200.2.0 255.255.255.0 172.16.5.4 200 name --GUEST_Wi-Fi--
ip route 192.168.51.44 255.255.255.255 Null0
ip ssh authentication-retries 2
ip ssh version 2
ip ssh server algorithm encryption aes128-ctr aes192-ctr aes256-ctr
ip ssh client algorithm encryption aes128-ctr aes192-ctr aes256-ctr
!
ip access-list standard ACL_CRPT_MARK
 permit 10.5.100.0 0.0.0.63
ip access-list standard ACL_NAT_SERVERS
 permit 10.5.96.0 0.0.0.255
ip access-list standard ACL_NAT_USERS
 permit 10.5.102.0 0.0.0.255
 permit 10.5.103.0 0.0.0.255
ip access-list standard ACL_NAT_WIFI
 permit 10.5.106.0 0.0.0.255
 permit 10.5.105.0 0.0.0.255
 permit 10.5.108.0 0.0.0.255
ip access-list standard ACL_PROD_MARKLINE
 permit 10.5.97.0 0.0.0.63
ip access-list standard ACL_PROD_TETRAPAK
 permit 10.5.99.0 0.0.0.63
ip access-list standard AUX
 permit 10.255.255.255
!
ip access-list extended ACL_TO_DMVPN
 deny   ip any 10.8.0.0 0.3.255.255 log
 deny   ip any 192.168.72.0 0.0.0.255 log
 permit ip any any
ip access-list extended FIREWALL
 permit ip object-group OBJ_BRANCHES object-group STATIC_ISP_IP
 permit icmp any any
 permit tcp any object-group STATIC_ISP_IP eq 2109
 permit object-group SVC_APS any object-group STATIC_ISP_IP
 permit object-group SVC_APS2 any object-group STATIC_ISP_IP
 permit object-group SVC_MAIL any any
 permit tcp object-group USER_APS2 object-group STATIC_ISP_IP eq 48608
 permit tcp any object-group STATIC_ISP_IP eq 443
 permit tcp any object-group STATIC_ISP_IP eq 7010 7020
 permit object-group SVC_ANDROMEDA any object-group STATIC_ISP_IP
 permit object-group SVC_IM any object-group STATIC_ISP_IP
 permit object-group SVC_VideoServer any object-group STATIC_ISP_IP
 permit object-group SVC_SYSADM any object-group STATIC_ISP_IP
 permit object-group SVC_POLYCOM any object-group STATIC_ISP_IP
 permit object-group SVC_IPTel any object-group STATIC_ISP_IP
 permit object-group VIDEO-TEMP any object-group STATIC_ISP_IP
 permit tcp any any eq 40001
 permit tcp any any eq 40002
 permit tcp any any eq 554
 permit tcp any any eq 53389
 deny   ip any any
ip access-list extended LOCAL_TRAFFIC
 permit ip any 192.168.0.0 0.0.255.255
 permit ip any 10.0.0.0 0.255.255.255
 permit ip any 172.16.0.0 0.15.255.255
ip access-list extended ROUTE_TO_ISP1
 permit ip object-group ROUTETOISP1 any
ip access-list extended ROUTE_TO_ISP2
 permit ip object-group ROUTETOISP2 any
!
!
ip prefix-list OUT_FROM_PS_PERM seq 10 permit 10.5.96.0/19
ip prefix-list OUT_FROM_PS_PERM seq 20 permit 192.168.48.0/22
ip prefix-list OUT_FROM_PS_PERM seq 30 permit 192.168.52.0/24
ip prefix-list OUT_FROM_PS_PERM seq 40 permit 192.168.55.0/25
ip sla 1
 icmp-echo 8.8.8.8 source-interface GigabitEthernet0/1
 threshold 2000
 timeout 3000
 frequency 10
ip sla schedule 1 life forever start-time now
ip sla 2
 icmp-echo 8.8.4.4 source-interface GigabitEthernet0/1
 threshold 2000
 timeout 3000
 frequency 10
ip sla schedule 2 life forever start-time now
ip sla 3
 icmp-echo 77.88.8.8 source-interface GigabitEthernet0/1
 threshold 2000
 timeout 3000
 frequency 10
ip sla schedule 3 life forever start-time now
ip sla 4
 icmp-echo 77.88.8.1 source-interface GigabitEthernet0/1
 threshold 2000
 timeout 3000
 frequency 10
ip sla schedule 4 life forever start-time now
ip sla 5
 icmp-echo 77.88.8.88 source-interface GigabitEthernet0/1
 threshold 2000
 timeout 3000
 frequency 10
ip sla schedule 5 life forever start-time now
ip sla 6
 icmp-echo 77.88.8.2 source-interface GigabitEthernet0/1
 threshold 2000
 timeout 3000
 frequency 10
ip sla schedule 6 life forever start-time now
logging origin-id hostname
logging facility local1
logging source-interface GigabitEthernet0/0.300
logging host 192.168.8.119 transport udp port 5544
logging host 10.4.244.4 transport udp port 515
ipv6 ioam timestamp
!
route-map MTS_LP permit 20
 set local-preference 1000
!
route-map RM_LOCAL permit 10
 match ip address 51
 set ip next-hop 46.146.210.254 31.173.105.57
!
route-map RM_LOCAL permit 20
 match ip address 52
 set ip next-hop 178.161.175.53 178.47.128.17
!
route-map RM_LOCAL permit 30
 match ip address 53
 set ip next-hop 78.85.13.1
!
route-map ISP_1 permit 10
 match ip address 1 ACL_PROD_MARKLINE ACL_PROD_TETRAPAK ACL_NAT_SERVERS ACL_NAT_USERS ACL_CRPT_MARK ACL_NAT_WIFI
 match interface GigabitEthernet0/1
!
route-map ISP_2 permit 10
 match ip address 1 ACL_PROD_MARKLINE ACL_PROD_TETRAPAK ACL_NAT_SERVERS ACL_NAT_USERS ACL_CRPT_MARK ACL_NAT_WIFI
 match interface GigabitEthernet0/2
!
route-map RM_TO_HUB permit 20
 match ip address prefix-list OUT_FROM_PS_PERM
!
route-map GLOBAL-ROUTING deny 20
 description --Deny_trafic_via_localnets--
 match ip address LOCAL_TRAFFIC
!
route-map GLOBAL-ROUTING permit 1001
 description --Route_to_isp1_about_local_device--
 match ip address ROUTE_TO_ISP1
 set ip default next-hop 46.146.210.254
!
route-map GLOBAL-ROUTING permit 1002
 description --Route_to_isp2_about_romote_device--
 match ip address ROUTE_TO_ISP2
 set ip default next-hop 192.168.51.252
!
!
snmp-server community lmTUEsk6Yvlv RO
access-list 1 deny   192.168.48.60
access-list 1 deny   192.168.48.144
access-list 1 deny   192.168.51.186
access-list 1 permit 192.168.0.0 0.0.255.255
access-list 1 permit 10.200.2.0 0.0.0.255
access-list 1 permit 10.5.112.0 0.0.0.31
access-list 51 remark IP address ISP1
access-list 51 permit 46.146.210.68
access-list 52 remark IP address ISP2
access-list 52 permit 178.47.128.18
!
radius server IZH-RDS002
 address ipv4 10.4.0.248 auth-port 1645 acct-port 1646
 timeout 3
 retransmit 2
 key hykFAA@Hg9X9fsokWh5q8wez#&^a9lIizldHKxlRer3RE7AbsTsJwdB^RESF$eJ0
!
radius server P11-RDS003
 address ipv4 10.1.122.248 auth-port 1645 acct-port 1646
 timeout 3
 retransmit 2
 key hykFAA@Hg9X9fsokWh5q8wez#&^a9lIizldHKxlRer3RE7AbsTsJwdB^RESF$eJ0
!
!
!
control-plane
!
 !
 !
 !
 !
!
mgcp behavior rsip-range tgcp-only
mgcp behavior comedia-role none
mgcp behavior comedia-check-media-src disable
mgcp behavior comedia-sdp-force disable
!
mgcp profile default
!
!
!
!
!
!
!
gatekeeper
 shutdown
!
!
 vstack
alias exec AUX telnet 10.255.255.255 2001 /vrf AUX
!
line con 0
 logging synchronous
 login authentication CONSOLE
line aux 0
 access-class AUX in vrf-also
 privilege level 15
 login authentication NPS
 rotary 1
 transport input telnet
 stopbits 1
line 2
 no activation-character
 no exec
 transport preferred none
 transport output lat pad telnet rlogin lapb-ta mop udptn v120 ssh
 stopbits 1
line vty 0 4
 exec-timeout 120 0
 logging synchronous
 login authentication NPS
 transport input ssh
line vty 5 15
 login authentication NPS
 transport input ssh
!
scheduler allocate 20000 1000
ntp source GigabitEthernet0/0.300
ntp update-calendar
ntp server 192.168.8.200
ntp server 192.168.8.201
!
end